# User documentation for autonomous skyscanner

## Connect to Raspberry Pi via wifi

ssid raspberry password skyscanner1

connect putty

host: 192.168.4.1 user: pi password: skyscanner

## Setting inifile

in directory /home/pi/Sky-Imager-Aggregator/src

edit file config.ini

### important items for autonomous running

phone number

change USB flash disk

## Monitoring Skyscanner

Miniatures are on address <http://wp2.pvforecast.cz/user/php/photos.php>

Logs are on address <http://wp2.pvforecast.cz/user/php/logs.php>